**RELAY BOARD MANAGER**

**REFERENCE**

**Welcome**

Welcome to use “Relay Board Manager”.

The software is produced by ICStation in 2014.

**Environment**

Operating system support:

Windows 7, Windows 7 Service Pack 1, Windows Server 2003 Service Pack 2, Windows Server 2008, Windows Server 2008 R2, Windows Server 2008 R2 SP1, Windows Vista Service Pack 1, Windows XP Service Pack 3

Hardware requirements:

Suggest the minimum requirements:

Pentium 1 GHz or faster, 512 MB RAM or greater  
Minimum disk space:

x86 – 850 MB

x64 – 2 GB









**Function**

Software is used to control relay module.

Applicable models are as follows:

ICSE012A , ICSE013A , ICSE014A

**Usage method**

1. Open the software “Relay Board manager”.
2. Select board.  
     
   Click “Finish” to ensure the selection.
3. Click “Open The Sele” to open the board select.  
   
4. In tab “Manul Mode” , click button to control the relay.  
   
5. In tab “Programer Mode” , you can write program as follows:  
   
6. Click “Start” to executive the program.  
   
7. You can operate the module as follows:  
   
8. The software can insert and save files as follows:  
   

**Thanks**

Thank you for reading . Have a nice time.